| ### Showing:
Annotations
Attributes
Diagrams
Facets
Instances
Properties
Source
Used by

Included schema DDMS-GeospatialCoverage.xsd

Namespace | urn:us:gov:ic:irm
Annotations | Change Log: 6/05/2007 (J. Pantella) -- Created pursuant to approved CR 2007-1. See also http://metadata.dod.mil/irs/DDMS/cm/CR/2007/DDMS-CR-2007-1. 1/3/2007 (J. Pantella) -- Modified version attribute to reflect that this is version 1.4.2. 6/30/2008 (D. Barclay) -- Made attribute osuffix optional (for CR 2008-5). 7/1/2008 (D. Barclay) -- Corrected "minVerticalExent" to "minVerticalExtent" 7/15/2008 (J. Pantella) -- Modified namespace to reflect DDMS 2.0. 1/4/2010 (P. Lunceford) -- Created DDMS 3.0. Implemented CR 2009-12 to add Security markings to GeospatialCoverageType and CR 2009-14 to make the value and qualifier of CompoundCountryCodeIdentifierType to be required.
Properties |
attribute form default: | qualified
element form default: | qualified
version: | 3.0.0
Schema location | DDMS-GeospatialCoverage.xsd

Element geospatialCoverage

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | GeospatialCoverageType
Properties |
content: | complex
Used by |
Complex Type | ResourceType
Model | GeospatialExtent
Children | GeospatialExtent
Instance |
    <geospatialCoverage SchemaguideSecurityAttributesOptionGroup="">
      <GeospatialExtent>{1,1}</GeospatialExtent>
    </geospatialCoverage>
Attributes |
QName | Type | Fixed | Default | Use | Annotation
--- | --- | --- | --- | --- | ---
SchemaguideSecurityAttributesOptionGroup | xsd:NMTOKEN |  |  | optional | This attribute is only a placeholder so that all the ISM attributes are not shown in the schemaGuide for every element. If you refer to the documentation of the attribute group it will say what attributes should be here.
Source |
    <xs:element name="geospatialCoverage" type="GeospatialCoverageType">
      <xs:annotation>
        <xs:appinfo>
          <mdr:definition>A geographic indication of one or more places or faciliies that relate to the resource. See DDMS Version 3.0 Geospatial Coverage.</mdr:definition>
        </xs:appinfo>
      </xs:annotation>
    </xs:element>
Schema location | DDMS-GeospatialCoverage.xsd

Element GeospatialCoverageType / GeospatialExtent

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | PlaceType
Properties |
content: | complex
Model | geographicIdentifier | boundingBox | boundingGeometry | postalAddress | verticalExtent
Children | boundingBox, boundingGeometry, geographicIdentifier, postalAddress, verticalExtent
Instance |
    <GeospatialExtent>
      <geographicIdentifier>{1,1}</geographicIdentifier>
      <boundingBox>{1,1}</boundingBox>
      <boundingGeometry>{1,1}</boundingGeometry>
      <postalAddress>{1,1}</postalAddress>
      <verticalExtent datum="" unitOfMeasure="">{1,1}</verticalExtent>
    </GeospatialExtent>
Source |
    <xs:element name="GeospatialExtent" type="PlaceType"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element geographicIdentifier

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Properties |
content: | complex
Used by |
Complex Type | PlaceType
Model | name{0,1} | region{0,1} | countryCode | facilityIdentifier
Children | countryCode, facilityIdentifier, name, region
Instance |
    <geographicIdentifier>
      <name>{0,1}</name>
      <region>{0,1}</region>
      <countryCode qualifier="" value="">{1,1}</countryCode>
      <facilityIdentifier beNumber="" osuffix="">{1,1}</facilityIdentifier>
    </geographicIdentifier>
Source |
    <xs:element name="geographicIdentifier">
      <xs:annotation>
        <xs:appinfo>
          <mdr:definition>Models a GML compliant geographic identifier.  See ISO 19115 EX_GeographicDescription.</mdr:definition>
        </xs:appinfo>
      </xs:annotation>
      <xs:complexType>
        <xs:choice maxOccurs="unbounded">
          <xs:element name="name" type="xs:string" minOccurs="0"/>
          <xs:element name="region" type="xs:string" minOccurs="0"/>
          <xs:element ref="ddms:countryCode"/>
          <xs:element ref="ddms:facilityIdentifier"/>
        </xs:choice>
      </xs:complexType>
    </xs:element>
Schema location | DDMS-GeospatialCoverage.xsd

Element geographicIdentifier / name

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | xs:string
Properties |
content: | simple
minOccurs: | 0
Source |
    <xs:element name="name" type="xs:string" minOccurs="0"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element geographicIdentifier / region

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | xs:string
Properties |
content: | simple
minOccurs: | 0
Source |
    <xs:element name="region" type="xs:string" minOccurs="0"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element countryCode

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | CompoundCountryCodeIdentifierType
Properties |
content: | complex
Used by |
Element | geographicIdentifier
Element Group | PostalAddressGroup
Attributes |
QName | Type | Fixed | Default | Use | Annotation
--- | --- | --- | --- | --- | ---
qualifier | icddms:CompoundCountryCodeQualifierType |  |  | required |
value | xs:NMTOKEN |  |  | required |
Source |
    <xs:element name="countryCode" type="CompoundCountryCodeIdentifierType"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element facilityIdentifier

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | FacilityIdentifierType
Properties |
content: | complex
Used by |
Element | geographicIdentifier
Attributes |
QName | Type | Fixed | Default | Use | Annotation
--- | --- | --- | --- | --- | ---
beNumber | xs:string |  |  | required |
osuffix | xs:string |  |  | optional |
Source |
    <xs:element name="facilityIdentifier" type="FacilityIdentifierType"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element boundingBox

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | BoundingBoxType
Properties |
content: | complex
Used by |
Complex Type | PlaceType
Model | WestBL , EastBL , SouthBL , NorthBL
Children | EastBL, NorthBL, SouthBL, WestBL
Instance |
    <boundingBox>
      <WestBL>{1,1}</WestBL>
      <EastBL>{1,1}</EastBL>
      <SouthBL>{1,1}</SouthBL>
      <NorthBL>{1,1}</NorthBL>
    </boundingBox>
Source |
    <xs:element name="boundingBox" type="BoundingBoxType">
      <xs:annotation>
        <xs:appinfo>
          <mdr:definition>Models a GML compliant bounding box.  See ISO 19115 EX_GeographicBoundingBox.</mdr:definition>
        </xs:appinfo>
      </xs:annotation>
    </xs:element>
Schema location | DDMS-GeospatialCoverage.xsd

Element BoundingBoxType / WestBL

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | xs:double
Properties |
content: | simple
Source |
    <xs:element name="WestBL" type="xs:double"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element BoundingBoxType / EastBL

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | xs:double
Properties |
content: | simple
Source |
    <xs:element name="EastBL" type="xs:double"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element BoundingBoxType / SouthBL

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | xs:double
Properties |
content: | simple
Source |
    <xs:element name="SouthBL" type="xs:double"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element BoundingBoxType / NorthBL

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | xs:double
Properties |
content: | simple
Source |
    <xs:element name="NorthBL" type="xs:double"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element boundingGeometry

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | BoundingGeometryType
Properties |
content: | complex
Used by |
Complex Type | PlaceType
Model | gml:Polygon | gml:Point
Children | gml:Point, gml:Polygon
Instance |
    <boundingGeometry>
      <gml:Polygon axisLabels="" gml:id="" srsDimension="" srsName="" uomLabels="">{1,1}</gml:Polygon>
      <gml:Point axisLabels="" gml:id="" srsDimension="" srsName="" uomLabels="">{1,1}</gml:Point>
    </boundingGeometry>
Source |
    <xs:element name="boundingGeometry" type="BoundingGeometryType">
      <xs:annotation>
        <xs:appinfo>
          <mdr:definition>Models a GML compliant bounding geometry.  See ISO 19115 EX_BoundingPolygon.</mdr:definition>
          <mdr:comment>Developer's Note: It is required that the srsName attribute be populated on a gml:Point or gml:Polygon element within the DDMS.  Recommended values for the attribute are:
            <!-- These Coordinate Reference System references are registered in the GSIP Governance Namespace on the DoD Metadata Registry. -->1) "http://metadata.dod.mil/mdr/ns/GSIP/crs/WGS84C_3D" -- representing World Geodetic System 1984 - Earth Centered, Earth Fixed (ECEF), where the X axis is mass center - equator/prime meridian, and the units are meters; the Y axis is mass center - equator/90° E, and the units are meters; and the Z axis is mass center - North Pole, and the units are meters.
    			OR
    			2) "http://metadata.dod.mil/mdr/ns/GSIP/crs/WGS84E_2D" -- representing World Geodetic System 1984 - Geographic, 2-Dimensional, where latitude is north positive, measured in degrees; and latitude is east positive, measured in degrees.
    			OR
    			3) "http://metadata.dod.mil/mdr/ns/GSIP/crs/WGS84E_3D" -- representing World Geodetic System 1984 - Geographic, 3-Dimensional, where latitude is north positive, measured in degrees; and latitude is east positive, measured in degrees; and height is height above ellipsoid, measured in meters.
    			See also: http://earth-info.nga.mil/GandG/publications/tr8350.2/tr8350_2.html.

    			For gml:pos elements populating the gml:Polygon/gml:exterior/gml:LinearRing/gml:pos element the following guidance should be followed:
    			1.	Latitude shall be in decimal degrees in the range -90° less than or equal to latitude greater than or equal to +90°.
    			2.	North latitudes shall be positive, south latitudes shall be negative.
    			3.	Longitude shall be in decimal degrees in the range -180° less than or equal to longitude greater than or equal to +180°; note that there are two equally acceptable values of longitude for the meridian opposite the prime meridian.
    			4.	East longitudes shall be positive, west longitudes shall be negative.
    			5.	Only the element gml:pos shall be used to encode a geographic point location as either:
    				a.	two decimal values in the order of latitude then longitude (no commas) when WGS84E_2D, or
    				b.	three decimal values in the order latitude, longitude and finally height above ellipsoid (no commas) when using the WGS84E_3D CRS.

    Developer's Note:  The srsName attribute is required on the Polygon element.  The Polygon/@srsName is the identifier for the CRS which is controlling for the child gml:pos elements.  It is important to note that the srsName attribute may also appear on the gml:pos elements, however given the current allowable CRSs above there is no need to repeat the information on the gml:pos elements thus the srsName attribute is optional and not required.  If the srsName does appear on the gml:pos elements then it must be the same as the value of the srsName attribute on the Polygon element.</mdr:comment>
        </xs:appinfo>
      </xs:annotation>
    </xs:element>
Schema location | DDMS-GeospatialCoverage.xsd

Element postalAddress

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Properties |
content: | complex
Used by |
Complex Type | PlaceType
Model | street{0,6} , city{0,1} , (state | province) , postalCode{0,1} , countryCode{0,1}
Children | city, countryCode, postalCode, province, state, street
Instance |
    <postalAddress>
      <street>{0,6}</street>
      <city>{0,1}</city>
      <postalCode>{0,1}</postalCode>
      <countryCode qualifier="" value="">{0,1}</countryCode>
    </postalAddress>
Source |
    <xs:element name="postalAddress">
      <xs:annotation>
        <xs:appinfo>
          <mdr:definition>Models a standalone postal address.</mdr:definition>
        </xs:appinfo>
      </xs:annotation>
      <xs:complexType>
        <xs:group ref="PostalAddressGroup"/>
      </xs:complexType>
    </xs:element>
Schema location | DDMS-GeospatialCoverage.xsd

Element PostalAddressGroup / street

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | xs:string
Properties |
content: | simple
minOccurs: | 0
maxOccurs: | 6
Source |
    <xs:element name="street" type="xs:string" minOccurs="0" maxOccurs="6"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element PostalAddressGroup / city

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | xs:string
Properties |
content: | simple
minOccurs: | 0
Source |
    <xs:element name="city" type="xs:string" minOccurs="0"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element PostalAddressGroup / state

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | xs:string
Properties |
content: | simple
Source |
    <xs:element name="state" type="xs:string"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element PostalAddressGroup / province

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | xs:string
Properties |
content: | simple
Source |
    <xs:element name="province" type="xs:string"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element PostalAddressGroup / postalCode

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | xs:string
Properties |
content: | simple
minOccurs: | 0
Source |
    <xs:element name="postalCode" type="xs:string" minOccurs="0"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element verticalExtent

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | VerticalExtentType
Properties |
content: | complex
Used by |
Complex Type | PlaceType
Model | MinVerticalExtent , MaxVerticalExtent
Children | MaxVerticalExtent, MinVerticalExtent
Instance |
    <verticalExtent datum="" unitOfMeasure="">
      <MinVerticalExtent datum="" unitOfMeasure="">{1,1}</MinVerticalExtent>
      <MaxVerticalExtent datum="" unitOfMeasure="">{1,1}</MaxVerticalExtent>
    </verticalExtent>
Attributes |
QName | Type | Fixed | Default | Use | Annotation
--- | --- | --- | --- | --- | ---
datum | VerticalDatumType |  |  | required |
unitOfMeasure | LengthMeasureType |  |  | required |
Source |
    <xs:element name="verticalExtent" type="VerticalExtentType">
      <xs:annotation>
        <xs:appinfo>
          <mdr:definition>Models a GML compliant vertical extent.  See ISO 19115 EX_VerticalExtent.</mdr:definition>
        </xs:appinfo>
      </xs:annotation>
    </xs:element>
Schema location | DDMS-GeospatialCoverage.xsd

Element MinVerticalExtent

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | VerticalDistanceType
Properties |
content: | complex
Used by |
Complex Type | VerticalExtentType
Attributes |
QName | Type | Fixed | Default | Use | Annotation
--- | --- | --- | --- | --- | ---
datum | VerticalDatumType |  |  | optional |
unitOfMeasure | LengthMeasureType |  |  | optional |
Source |
    <xs:element name="MinVerticalExtent" type="VerticalDistanceType"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element MaxVerticalExtent

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | VerticalDistanceType
Properties |
content: | complex
Used by |
Complex Type | VerticalExtentType
Attributes |
QName | Type | Fixed | Default | Use | Annotation
--- | --- | --- | --- | --- | ---
datum | VerticalDatumType |  |  | optional |
unitOfMeasure | LengthMeasureType |  |  | optional |
Source |
    <xs:element name="MaxVerticalExtent" type="VerticalDistanceType"/>
Schema location | DDMS-GeospatialCoverage.xsd

Complex Type GeospatialCoverageType

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Used by |
Element | geospatialCoverage
Model | GeospatialExtent
Children | GeospatialExtent
Attributes |
QName | Type | Fixed | Default | Use | Annotation
--- | --- | --- | --- | --- | ---
SchemaguideSecurityAttributesOptionGroup | xsd:NMTOKEN |  |  | optional | This attribute is only a placeholder so that all the ISM attributes are not shown in the schemaGuide for every element. If you refer to the documentation of the attribute group it will say what attributes should be here.
Source |
    <xs:complexType name="GeospatialCoverageType">
      <xs:annotation>
        <xs:appinfo>
          <mdr:definition>Type used to model the geospatialCoverage element.</mdr:definition>
        </xs:appinfo>
      </xs:annotation>
      <xs:sequence>
        <xs:element name="GeospatialExtent" type="PlaceType"/>
      </xs:sequence>
      <xs:attributeGroup ref="ICISM:SecurityAttributesOptionGroup"/>
    </xs:complexType>
Schema location | DDMS-GeospatialCoverage.xsd

Complex Type PlaceType

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Used by |
Element | GeospatialCoverageType/GeospatialExtent
Model | geographicIdentifier | boundingBox | boundingGeometry | postalAddress | verticalExtent
Children | boundingBox, boundingGeometry, geographicIdentifier, postalAddress, verticalExtent
Source |
    <xs:complexType name="PlaceType">
      <xs:choice maxOccurs="unbounded">
        <xs:element ref="geographicIdentifier"/>
        <xs:element ref="boundingBox"/>
        <xs:element ref="boundingGeometry"/>
        <xs:element ref="postalAddress"/>
        <xs:element ref="verticalExtent"/>
      </xs:choice>
    </xs:complexType>
Schema location | DDMS-GeospatialCoverage.xsd

Complex Type CompoundCountryCodeIdentifierType

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Used by |
Element | countryCode
Attributes |
QName | Type | Fixed | Default | Use | Annotation
--- | --- | --- | --- | --- | ---
qualifier | icddms:CompoundCountryCodeQualifierType |  |  | required |
value | xs:NMTOKEN |  |  | required |
Source |
    <xs:complexType name="CompoundCountryCodeIdentifierType">
      <xs:attribute name="qualifier" type="icddms:CompoundCountryCodeQualifierType" use="required"/>
      <xs:attribute name="value" type="xs:NMTOKEN" use="required"/>
    </xs:complexType>
Schema location | DDMS-GeospatialCoverage.xsd

Complex Type FacilityIdentifierType

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Used by |
Element | facilityIdentifier
Attributes |
QName | Type | Fixed | Default | Use | Annotation
--- | --- | --- | --- | --- | ---
beNumber | xs:string |  |  | required |
osuffix | xs:string |  |  | optional |
Source |
    <xs:complexType name="FacilityIdentifierType">
      <xs:attribute name="beNumber" type="xs:string" use="required">
        <xs:annotation>
          <xs:appinfo>
            <mdr:definition>(GMI:BE_NUMBER, 1.0) Uniquely identifies the installation of the facility.  The BE_NUMBER is generated based on the value input for the COORD to determine the appropriate World Area Code (WAC), the system assigned record originator and a one-up-number.  Pos. 1-4, World Area Code (WAC).  Pos. 5,  A hyphen, '-', or an 'E', in the fifth position indicates that position-6 will contain values 0-9.  Alternately, the fifth position may contain the first of a two-character system assigned record originator code, position-6 will then contain the second character of the system assigned record originator code.  Pos. 6,  May contain the second character of the  system assigned record originator code, the one-up-number series will then begin in position seven, and range from  0001-9909.  If the one-up-number series begins in postion 6, this position will contain the first of a five-position one-up-number, i.e., 00001-99999.Pos. 7-10,  A one-up-number series.  Depending on the content of position 5, the series may have begun in position 6 and have a range of 00001-99999.  Or, have begun in position 7 and have a range from 0001-9999.</mdr:definition>
          </xs:appinfo>
        </xs:annotation>
      </xs:attribute>
      <xs:attribute name="osuffix" type="xs:string" use="optional">
        <xs:annotation>
          <xs:appinfo>
            <mdr:definition>(GMI:OSUFFIX, 1.0) Uniquely identifies a facility or demographic area in conjunction with a BE_NUMBER.  Pos. 1-2.  SYSTEM ASSIGNED RECORD_ORIGINATOR.  The organization creating the facility or demographic area.  DIA installation records created prior to IDB generation of OSUFFIX contain DD.Pos. 3-5  A one-up number.</mdr:definition>
          </xs:appinfo>
        </xs:annotation>
      </xs:attribute>
    </xs:complexType>
Schema location | DDMS-GeospatialCoverage.xsd

Complex Type BoundingBoxType

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Used by |
Element | boundingBox
Model | WestBL , EastBL , SouthBL , NorthBL
Children | EastBL, NorthBL, SouthBL, WestBL
Source |
    <xs:complexType name="BoundingBoxType">
      <xs:annotation>
        <xs:appinfo>
          <mdr:definition>Type that defines a GML compliant bounding box.  See ISO 19115 EX_GeographicBoundingBox.</mdr:definition>
        </xs:appinfo>
      </xs:annotation>
      <xs:sequence>
        <xs:element name="WestBL" type="xs:double"/>
        <xs:element name="EastBL" type="xs:double"/>
        <xs:element name="SouthBL" type="xs:double"/>
        <xs:element name="NorthBL" type="xs:double"/>
      </xs:sequence>
    </xs:complexType>
Schema location | DDMS-GeospatialCoverage.xsd

Complex Type BoundingGeometryType

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Used by |
Element | boundingGeometry
Model | gml:Polygon | gml:Point
Children | gml:Point, gml:Polygon
Source |
    <xs:complexType name="BoundingGeometryType">
      <xs:annotation>
        <xs:appinfo>
          <mdr:definition>Type that defines a GML compliant bounding geometry.  See ISO 19115 EX_BoundingPolygon.</mdr:definition>
          <mdr:comment>Developer's Note: It is required that the srsName attribute be populated on a gml:Point or gml:Polygon element within the DDMS.  Recommended values for the attribute are:
            <!-- These Coordinate Reference System references are registered in the GSIP Governance Namespace on the DoD Metadata Registry. -->1) "http://metadata.dod.mil/mdr/ns/GSIP/crs/WGS84C_3D" -- representing World Geodetic System 1984 - Earth Centered, Earth Fixed (ECEF), where the X axis is mass center - equator/prime meridian, and the units are meters; the Y axis is mass center - equator/90° E, and the units are meters; and the Z axis is mass center - North Pole, and the units are meters.
    			OR
    			2) "http://metadata.dod.mil/mdr/ns/GSIP/crs/WGS84E_2D" -- representing World Geodetic System 1984 - Geographic, 2-Dimensional, where latitude is north positive, measured in degrees; and latitude is east positive, measured in degrees.
    			OR
    			3) "http://metadata.dod.mil/mdr/ns/GSIP/crs/WGS84E_3D" -- representing World Geodetic System 1984 - Geographic, 3-Dimensional, where latitude is north positive, measured in degrees; and latitude is east positive, measured in degrees; and height is height above ellipsoid, measured in meters.
    			See also: http://earth-info.nga.mil/GandG/publications/tr8350.2/tr8350_2.html.

    			For gml:pos elements populating the gml:Polygon/gml:exterior/gml:LinearRing/gml:pos element the following guidance should be followed:
    			1.	Latitude shall be in decimal degrees in the range -90° less than or equal to latitude greater than or equal to +90°.
    			2.	North latitudes shall be positive, south latitudes shall be negative.
    			3.	Longitude shall be in decimal degrees in the range -180° less than or equal to longitude greater than or equal to +180°; note that there are two equally acceptable values of longitude for the meridian opposite the prime meridian.
    			4.	East longitudes shall be positive, west longitudes shall be negative.
    			5.	Only the element gml:pos shall be used to encode a geographic point location as either:
    				a.	two decimal values in the order of latitude then longitude (no commas) when WGS84E_2D, or
    				b.	three decimal values in the order latitude, longitude and finally height above ellipsoid (no commas) when using the WGS84E_3D CRS.

    Developer's Note:  The srsName attribute is required on the Polygon element.  The Polygon/@srsName is the identifier for the CRS which is controlling for the child gml:pos elements.  It is important to note that the srsName attribute may also appear on the gml:pos elements, however given the current allowable CRSs above there is no need to repeat the information on the gml:pos elements thus the srsName attribute is optional and not required.  If the srsName does appear on the gml:pos elements then it must be the same as the value of the srsName attribute on the Polygon element.</mdr:comment>
        </xs:appinfo>
      </xs:annotation>
      <xs:choice maxOccurs="unbounded">
        <xs:element ref="gml:Polygon"/>
        <xs:element ref="gml:Point"/>
      </xs:choice>
    </xs:complexType>
Schema location | DDMS-GeospatialCoverage.xsd

Complex Type VerticalExtentType

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Used by |
Element | verticalExtent
Model | MinVerticalExtent , MaxVerticalExtent
Children | MaxVerticalExtent, MinVerticalExtent
Attributes |
QName | Type | Fixed | Default | Use | Annotation
--- | --- | --- | --- | --- | ---
datum | VerticalDatumType |  |  | required |
unitOfMeasure | LengthMeasureType |  |  | required |
Source |
    <xs:complexType name="VerticalExtentType">
      <xs:annotation>
        <xs:appinfo>
          <mdr:definition>Type that defines a GML compliant vertical extent.  See ISO 19115 EX_VerticalExtent.</mdr:definition>
        </xs:appinfo>
      </xs:annotation>
      <xs:sequence>
        <xs:element ref="MinVerticalExtent"/>
        <xs:element ref="MaxVerticalExtent"/>
      </xs:sequence>
      <xs:attribute name="unitOfMeasure" type="LengthMeasureType" use="required"/>
      <xs:attribute name="datum" type="VerticalDatumType" use="required"/>
    </xs:complexType>
Schema location | DDMS-GeospatialCoverage.xsd

Complex Type VerticalDistanceType

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Type | extension of xs:double
Used by |
Elements | MaxVerticalExtent, MinVerticalExtent
Attributes |
QName | Type | Fixed | Default | Use | Annotation
--- | --- | --- | --- | --- | ---
datum | VerticalDatumType |  |  | optional |
unitOfMeasure | LengthMeasureType |  |  | optional |
Source |
    <xs:complexType name="VerticalDistanceType">
      <xs:simpleContent>
        <xs:extension base="xs:double">
          <xs:attribute name="unitOfMeasure" type="LengthMeasureType" use="optional"/>
          <xs:attribute name="datum" type="VerticalDatumType" use="optional"/>
        </xs:extension>
      </xs:simpleContent>
    </xs:complexType>
Schema location | DDMS-GeospatialCoverage.xsd

Attribute CompoundCountryCodeIdentifierType / @qualifier

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Type | icddms:CompoundCountryCodeQualifierType
Properties |
use: | required
Facets |
enumeration | urn:us:gov:ic:cvenum:irm:coverage:fips:digraph:v1 |
enumeration | urn:us:gov:ic:cvenum:irm:coverage:iso3166:digraph:v1 |
enumeration | urn:us:gov:ic:cvenum:irm:coverage:iso3166:numeric:v1 |
enumeration | urn:us:gov:ic:cvenum:irm:coverage:iso3166:trigraph:v1 |
Used by |
Complex Type | CompoundCountryCodeIdentifierType
Source |
    <xs:attribute name="qualifier" type="icddms:CompoundCountryCodeQualifierType" use="required"/>
Schema location | DDMS-GeospatialCoverage.xsd

Attribute CompoundCountryCodeIdentifierType / @value

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Type | xs:NMTOKEN
Properties |
use: | required
Used by |
Complex Type | CompoundCountryCodeIdentifierType
Source |
    <xs:attribute name="value" type="xs:NMTOKEN" use="required"/>
Schema location | DDMS-GeospatialCoverage.xsd

Attribute FacilityIdentifierType / @beNumber

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Type | xs:string
Properties |
use: | required
Used by |
Complex Type | FacilityIdentifierType
Source |
    <xs:attribute name="beNumber" type="xs:string" use="required">
      <xs:annotation>
        <xs:appinfo>
          <mdr:definition>(GMI:BE_NUMBER, 1.0) Uniquely identifies the installation of the facility.  The BE_NUMBER is generated based on the value input for the COORD to determine the appropriate World Area Code (WAC), the system assigned record originator and a one-up-number.  Pos. 1-4, World Area Code (WAC).  Pos. 5,  A hyphen, '-', or an 'E', in the fifth position indicates that position-6 will contain values 0-9.  Alternately, the fifth position may contain the first of a two-character system assigned record originator code, position-6 will then contain the second character of the system assigned record originator code.  Pos. 6,  May contain the second character of the  system assigned record originator code, the one-up-number series will then begin in position seven, and range from  0001-9909.  If the one-up-number series begins in postion 6, this position will contain the first of a five-position one-up-number, i.e., 00001-99999.Pos. 7-10,  A one-up-number series.  Depending on the content of position 5, the series may have begun in position 6 and have a range of 00001-99999.  Or, have begun in position 7 and have a range from 0001-9999.</mdr:definition>
        </xs:appinfo>
      </xs:annotation>
    </xs:attribute>
Schema location | DDMS-GeospatialCoverage.xsd

Attribute FacilityIdentifierType / @osuffix

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Type | xs:string
Properties |
use: | optional
Used by |
Complex Type | FacilityIdentifierType
Source |
    <xs:attribute name="osuffix" type="xs:string" use="optional">
      <xs:annotation>
        <xs:appinfo>
          <mdr:definition>(GMI:OSUFFIX, 1.0) Uniquely identifies a facility or demographic area in conjunction with a BE_NUMBER.  Pos. 1-2.  SYSTEM ASSIGNED RECORD_ORIGINATOR.  The organization creating the facility or demographic area.  DIA installation records created prior to IDB generation of OSUFFIX contain DD.Pos. 3-5  A one-up number.</mdr:definition>
        </xs:appinfo>
      </xs:annotation>
    </xs:attribute>
Schema location | DDMS-GeospatialCoverage.xsd

Attribute VerticalDistanceType / @unitOfMeasure

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Type | LengthMeasureType
Properties |
use: | optional
Facets |
enumeration | Meter |
enumeration | Kilometer |
enumeration | Foot |
enumeration | StatuteMile |
enumeration | NauticalMile |
enumeration | Fathom |
enumeration | Inch |
Used by |
Complex Type | VerticalDistanceType
Source |
    <xs:attribute name="unitOfMeasure" type="LengthMeasureType" use="optional"/>
Schema location | DDMS-GeospatialCoverage.xsd

Attribute VerticalDistanceType / @datum

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Type | VerticalDatumType
Properties |
use: | optional
Facets |
enumeration | MSL |
enumeration | AGL |
enumeration | HAE |
Used by |
Complex Type | VerticalDistanceType
Source |
    <xs:attribute name="datum" type="VerticalDatumType" use="optional"/>
Schema location | DDMS-GeospatialCoverage.xsd

Attribute VerticalExtentType / @unitOfMeasure

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Type | LengthMeasureType
Properties |
use: | required
Facets |
enumeration | Meter |
enumeration | Kilometer |
enumeration | Foot |
enumeration | StatuteMile |
enumeration | NauticalMile |
enumeration | Fathom |
enumeration | Inch |
Used by |
Complex Type | VerticalExtentType
Source |
    <xs:attribute name="unitOfMeasure" type="LengthMeasureType" use="required"/>
Schema location | DDMS-GeospatialCoverage.xsd

Attribute VerticalExtentType / @datum

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Type | VerticalDatumType
Properties |
use: | required
Facets |
enumeration | MSL |
enumeration | AGL |
enumeration | HAE |
Used by |
Complex Type | VerticalExtentType
Source |
    <xs:attribute name="datum" type="VerticalDatumType" use="required"/>
Schema location | DDMS-GeospatialCoverage.xsd

Element Group PostalAddressGroup

Namespace | http://metadata.dod.mil/mdr/ns/DDMS/3.0/
Diagram |
Used by |
Element | postalAddress
Model | street{0,6} , city{0,1} , (state | province) , postalCode{0,1} , countryCode{0,1}
Children | city, countryCode, postalCode, province, state, street
Source |
    <xs:group name="PostalAddressGroup">
      <xs:annotation>
        <xs:appinfo>
          <mdr:definition>Group of entities used in the ddms:postalAddress element.</mdr:definition>
        </xs:appinfo>
      </xs:annotation>
      <xs:sequence>
        <xs:element name="street" type="xs:string" minOccurs="0" maxOccurs="6"/>
        <xs:element name="city" type="xs:string" minOccurs="0"/>
        <xs:choice minOccurs="0">
          <xs:element name="state" type="xs:string"/>
          <xs:element name="province" type="xs:string"/>
        </xs:choice>
        <xs:element name="postalCode" type="xs:string" minOccurs="0"/>
        <xs:element ref="ddms:countryCode" minOccurs="0"/>
      </xs:sequence>
    </xs:group>
Schema location | DDMS-GeospatialCoverage.xsd