| ### Showing:
Annotations
Attributes
Diagrams
Instances
Properties
Source

Element ntk:Access

Namespace | urn:us:gov:ic:ntk
Annotations | A way of describing a formalized Need to Know required for a document. NTK requires being inside a schema that implements ISM therefore some element in the implementing schema MUST have ism:ISMRootNodeAttributeGroup and ism:ResourceNodeAttributeGroup since both of those are required for a valid ISM implementation. In addition the root node of the implementing schema must have ntk:NTKRootNodeAttributeGroup specified.
Diagram |
Type | ntk:AccessType
Properties |
content: | complex
Model | ALL(ntk:AccessIndividualList{0,1} ntk:AccessGroupList{0,1} ntk:AccessProfileList{0,1})
Children | ntk:AccessGroupList, ntk:AccessIndividualList, ntk:AccessProfileList
Instance |
    <ntk:Access ntk:externalReference="" SchemaguideSecurityAttributesGroup="" xmlns:ntk="urn:us:gov:ic:ntk">
      <ntk:AccessIndividualList>{0,1}</ntk:AccessIndividualList>
      <ntk:AccessGroupList>{0,1}</ntk:AccessGroupList>
      <ntk:AccessProfileList SchemaguideSecurityAttributesGroup="">{0,1}</ntk:AccessProfileList>
    </ntk:Access>
Attributes |
QName | Type | Fixed | Default | Use | Annotation
--- | --- | --- | --- | --- | ---
SchemaguideSecurityAttributesGroup | xsd:NMTOKEN |  |  | optional | This attribute is only a placeholder so that all the ISM attributes are not shown in the schemaGuide for every element. If you refer to the documentation of the attribute group it will say what attributes should be here.
ntk:externalReference | xsd:boolean |  |  | optional |
Source |
    <xsd:element name="Access" type="ntk:AccessType">
      <xsd:annotation>
        <xsd:documentation>
          <p xmlns="http://www.w3.org/1999/xhtml" ism:ownerProducer="USA" ism:classification="U">A way of describing a formalized Need to Know required for a document. NTK requires being inside a schema that implements ISM therefore some element in the implementing schema MUST have ism:ISMRootNodeAttributeGroup and ism:ResourceNodeAttributeGroup since both of those are required for a valid ISM implementation. In addition the root node of the implementing schema must have ntk:NTKRootNodeAttributeGroup specified.</p>
        </xsd:documentation>
      </xsd:annotation>
    </xsd:element>
Schema location | IC-NTK.xsd

## This document has been approved for Public Release by the Office of the Director of National Intelligence. See 'Distribution Notice' for details. Click Here