| ### Showing:
Attributes
Diagrams
Source

Attribute Group ntk:NtkPortionAccessGroup

Namespace | urn:us:gov:ic:ntk
Diagram |
Attributes |
QName | Type | Fixed | Default | Use | Annotation
--- | --- | --- | --- | --- | ---
ntk:access | ntk:NtkPortionAccessType |  |  | optional | Used for portion marking access requirements with a format of a namespace-prefix followed by sets of key-value pairs. The '|' character is used to separate the key-value pairs and the '^' character is used to join keys with their values. Multiple namespace-prefixed sets can be used. For example: ntk:access="namespace1|key1^value1|key2^value1|key2^value2" ntk:access="namespace1|key1^value1 namespace2|key1^value1|key2^value2" ntk:access="namespace1|key1^value1|key2^val2 namespace1|key1^value3"
Source |
    <xsd:attributeGroup name="NtkPortionAccessGroup">
      <xsd:attribute ref="ntk:access"/>
    </xsd:attributeGroup>
Schema location | IC-NTK.xsd

## This document has been approved for Public Release by the Office of the Director of National Intelligence. See 'Distribution Notice' for details. Click Here